**Jebel Dhanna Draft Restrictions:**

•   Channel depth is 14.00 Meters (Chart Datum).

•   Vessels drawing 13.4 Meters draft may sail any time.

•   Vessels drawing 13.7 Meters draft will rarely have to wait for the tide.

•   Vessels drawing 14.0 Meters draft will usually have to wait for the tide.

•   Vessels drawing 14.3 Meters draft will always have to wait for the tide.

•   Under keel clearance required as per regulations below;

•   1.22 Meters for Vessel DWT between 100,000 to 250,000 Mtons.

•   1.52 Meters for Vessel DWT between 250,000 and 350,000 Mtons.

•   1.83 Meters for Vessel DWT over 350,000 Mtons.

•   The Highest Average spring high tide is 2.0 Meters above Chart Datum, the Lowest Average spring tide is 1.0 Meters above Chart Datum.

**Quote:**

4.1.17 Under Keel Clearance

Subject to limitations upon draft, under keel clearance and extreme adverse weather conditions, vessels may enter or leave at any time during the day or night.

To ensure safe channel passage: **(**Channel depth is 14.0 meter at CD**)**, a minimum under keel clearance is required for all ships entering or leaving the port when deep loaded, as follows

A Up to 100,000 SDWT 0.92 m / 3 Ft

B Up to 250,000 SDWT 1.22 m / 4 Ft

C Up to 350,000 SDWT 1.52 m / 5 Ft

D Over 350,000 SDWT 1.83 m / 6 Ft

Best regards,

**Capt. Noman Siddiqui**

Harbour Master

JD/Ruwais Port

Ph No. +971 2 60 21771

Fax No. +971 2 60 21700

Mobile No. +971 50 7129381

[www.adppa.ae](http://www.adppa.ae/)

**Unquote:**